* 1. **Knapp Connector RICON S**

Manufacturing of a choose the connection with Knapp connecting system

choose the dimension to materials as a connection. The connection is made select visibility in accordance with the manufacturer's instruction manual. Select if bearing loads occur

The RICON S connecting system consists of two identical, 5 mm thick, hot-dip galvanized sheet steel plates. The system can optionally be combined with a locking clip made of 2 mm thick, stainless spring steel to withstand uplift loads. The fastening is done using self-tapping fully threaded screws Ø 8 mm or Ø 10 mm.

The connector is available in three different versions: VS- with welded collar bolt, VK- with screwed collar bolt, EK- with adjustable collar bolt.

Quantity: …………………. Unit Price: ……………………… Total Price: ……………………..

* 1. **Structural connection with connecting systems**

Manufacturing of choose the connection to materials as a connection. The connection is made select visibility in accordance with the manufacturer's instruction manual. Select if bearing loads occur

Base of planning:

Knapp Connector

Choose a connector size

The RICON S connecting system consists of two identical, 5 mm thick, hot-dip galvanized sheet steel plates. The system can optionally be combined with a locking clip made of 2 mm thick, stainless spring steel to withstand uplift loads. The fastening is done using self-tapping fully threaded screws Ø 8 mm or Ø 10 mm.

The connector is available in three different versions: VS- with welded collar bolt, VK- with screwed collar bolt, EK- with adjustable collar bolt.

Or equivalent.

Offered product: ………………………………………………………………………….

Quantity: …………………. Unit Price: ……………………… Total Price: ……………………..